KIEAE Journal, Vol. 20, No. 1, Jan. 2020, pp.1-10.

KIEAE Journal

Korea Institute of Ecological Architecture and Environment

106

한국생태환경건축학회 논문의 한글 제목 표시 부분 (나눔고딕 B14)

- 한국 지역 아파트단지를 중심으로 - (나눔고딕 B12) (없을 경우 행 생략)

This is English Article Title Space of Korea Institute of Ecological Architecture and Environment (12point)

- Focused on Apartment in Korea & This is Small Title - (10point) (없을 경우 행 생략)

궁서체10*ㆍまつしたこうのすけ**ㆍ劉 德華***ㆍ나논문****

Seng-Tae Han*ㆍSung Jae Park**ㆍKounosuke Matsusita***ㆍAndy Lau****

* Graduate Student, Dept. of Architectural Engineering, HanKook National Univ., South Korea (captivator@kieie.org)

** Coauthor, Undergraduate Student, Dept. of Architectural Engineering, Japan Abcd Univ., Japan (artist123@quartro.edu)

*** Coauthor, Researcher, Dept. of Architectural Engineering, Japan Abcd Univ., Japan (artist456@quartro.edu)

**** Corresponding author, Professor, Dept. of Architecture, Qindao Technological Univ., China (antris@kieie.org)

	KIEAE Journal, Vol. 20, No. 1, Feb. 2020

ⓒ 2020. Korea Institute of Ecological Architecture and Environment all rights reserved.

한국생태환경건축학회 논문집 제목 표시 부분입니다

한국생태환경건축학회 논문집 저자명 표시 부분입니다

pISSN 2288‐968X, eISSN 2288‐9698

http://dx.doi.org/10.12813/kieae.2020.20.2.065

ABSTRACT

KEYWORD

Purpose: Highlighting the significant impacts of shading on PV efficiencies were presented. The literature indicates that even the partial shading of a single cell can greatly drop the entire module voltage and power efficiency. The MMP tracking approaches were also reviewed in this study. Both conventional and advanced soft computing methods such as ANN, FLC and EA were described for the proper tracking of MMP under shaded conditions. This paper would be the basic significant impacts of shading on PV efficiencies were presented. The literature indicates that even the partial shading of a single cell can greatly drop the entire module voltage and power efficiency. The MMP tracking approaches were also reviewed in this study. Method: Both conventional and advanced soft computing methods such as ANN, FLC and EA were described for the proper tracking of MMP under shaded conditions. The MMP tracking approaches were also reviewed in this study. Both conventional and advanced soft computing methods such as ANN, FLC and EA were described for the proper tracking of MMP under shaded conditions. Result: This paper would be the basic source and the comprehensive information associated with the shading effects and relevant MPP tracking technique.

ⓒ 2020. KIEAE all rights reserved.

생태환경

학회키워드

아파트단지

Ecological

Keyword abc

Apartment Complex

ACCEPTANCE INFO

Received May. 3, 2020

Final revision received Jul. 23, 2020

Accepted Aug. 20, 2020

1. 서론

1.1. 연구의 배경 및 목적

따라서 거주자들은 주거환경이 범죄로부터 안전하기를 원하고 주거공간의 안정성 확보를 위한 다양한 대책 마련에 노력하고 있다. 범죄 및 범죄 불안 감소를 위한 대표적 대책 방안으로 주목받는 것이 있다. 아울러 CPTED를 이용한 연구는 많이 있으나 2006년 이후의 아파트단지만을 대상으로 연구된 것은 없어서 근래 지어진 아파트의 동향을 파악하는데 유용할 수 있을 것으로 본다.

이에 본 연구는 아파트단지 주변 주요 공간을 조사하고 분석함으로써 아파트들에서 범죄 예방 환경의 수준을 파악하고, 안전한 주거단지가 되기 위하여 개선이 필요한 부분은 어떤 것이 있는지 살펴봄으로써 안전한 주거단지가 될 수 있는 방안을 모색해 보고자 한다.

1.2. 연구의 방법 및 범위

이후 완공된 아파트 단지를 조사 대상으로 선정하여 각각의 단지 마다 CPTED 적용실태를 조사하고자 한다. 그리고 선행 연구 및 각 단지의 현장 조사를 바탕으로 CPTED의 적용 실태를 분석하고, 안전한 아파트 단지 계획을 위한 대안 및 개선 계획 방안을 제시하고자 한다. 아울러 본 연구의 범위는 대전지역으로 한정하였으며 조사대상 단지는 2006년 이후 지어진 18개 아파트단지를 대상으로 임의로 선정하였다[1].

1992년 건설교통부에서 ‘방범설계를 위한 지침’을 배부하였으며, 2005년 3월 CPTED 추진 계획을 수립 및 시행, 2009년 KS A8801, 8802, 8810 등의 국가표준들이 마련되었다.

대전광역시 유성구 가정로 201-219 일대.

2. 생태환경의 개념과 이론

2.1. 선행연구 고찰

1) 일반적인 사항

따라서 거주자들은 주거환경이 범죄로부터 안전하기를 원하고 주거공간의 안정성 확보를 위한 다양한 대책 마련에 노력하고 있다. 이에 본 연구는 아파트단지 주변 주요 공간을 조사하고 분석함으로써 아파트들에서 범죄 예방 환경의 수준을 파악해 보고자 한다.

2) 고려사항

2.2. 논문작성의 6가지 원리

권리를 주장할 수 있는 가상의 영역을 말하는 것이다. 또한, 영역성 강화는 실제적, 가설물이나 공공장소가 지속적으로 이용될 수 있도록 하는 것이다.

3. 조사대상 및 분석

3.1. 조사대상지 선정

지침이 수립되고 배포가 이루어진 시점 이후인 2006년 이후에 완공된 대전지역에 있다[2]. 본 연구에서는 49개 단지 중 무작위로 18개 단지를 대상지로 선정하였다.

국토교통부 고시 제 2014-302호 ｢건설공사 안전관리 지침｣, 국토교통부 고시 제2016-718호 ｢건설공사 안전관리업무수행 지침｣.

3.2. 한국의 미

그림을 도출하였다. 범죄불안심리에 영향을 미치는 물리적 환경요소를 Table 1.과 같이 설정하고 평가항목을 작성하였다. 단, 분석과정 중에서 중복되는 물리적 환경 요소들은  CPTED 6가지 조건을 재설정하였다[3].

Table 1. Container box dimension for ISO

ISO Standard		20ft	20ft HC*	40ft	40ft HC*
Out-scale (mm)	Length	6,058	6,058	12,192	12,192
	Width	2,438	2,438	2,438	2,438
	Hight	2,591	2,896	2,591	2,896
In-scale (mm)	Length	5,898	5,898	12,032	12,032
	Width	2,350	2,350	2,350	2,350
	Hight	2,390	2,695	2,390	2,695
*HC: High Cube

Fig. 1. Comparison of monthly electricity use for space cooling

Table 2. Case of twin module

Type name	Front Elevation	Isometric
Type 2-1
Type 2-2
Type 2-3
Type 2-4

Fig. 1.에 따르면 외부인의 접근에 제약이 없는 경우가 많았다. 따라서 보행자 출입구에도 CCTV 또는 경비실을 설치하여 외부인의 접근을 통제를 강 운영의 허점으로 인한 범죄유발의 위험도 간과할 수 없어 보였다(Eq. 1).

Closed-circuit Television.

[eqn: int _{t} ^{t prime} {LEFT ( x ^{2} +sin theta RIGHT ) dx} + alpha]	(Eq. 1)

출입구에 경비실이 설치된 단지는 3곳뿐이었으며 E단지에 1개, P단지에 1개, Q단지에 3개 있었다. 단지입수의 물리적 환경을 조사한 결과를 종합해 보면 (Eq. 2)와 같고, Q단지가 CPTED 기본원리에 가장 부합된 출입구를 본다[4][5].

[eqn: y= {c ^{2}} over {t} +6.02 TIMES10 ^{18} +t]	(Eq. 2)

아파트 단지 외벽의 상태는 1개 단지를 제외하고는 양호하였다. Table 2.에서 확인되는 바와 같이, 필로티 공간이 협소하고 어두워서 감시가 용이하지 않아[2-3][6] 은폐공간으로 보이는 곳은 4곳이었다. 대부분의 단지는 도로가 순환되거나, 출입구와 연결이 되었으며 1개 단지에서는 막다른 길이 있었다[4-6].

4. 결론

결론적 문장 부분으로 감시가 잘 안 되는 자전거보관소나 필로티에도 CCTV 설치가 되어야 할 필요가 있는 경우가 많았다.

Acknowledgement

본 연구는 2020년 한국대학 학술 연구 지원으로 이루어졌습니다.

References

[1] 홍길동, 환경설계를 통한 범죄예방, 한국: 한국학술정보(주), 2006, p.99. // (G.H. Hong, Crime Prevention Through Evidential Design, Korea: Korea Academic Information Inc., 2006, p.99.)

[2] 국토교통부, 건축물의 설비기준에 관한 규칙, 국토교통부 고시 제2017-467호 // (Ministry of Land, Infrastructure and Transport, Rules on the Building Equipment Standards, Koream MOLIT, 2017)

[3] 박소영 외 3인, 환경설계(CPTED)를 활용한 도시범죄 예방, 한국: 생활학회지, 제17권 제4호, 2010.04, pp.20-22. // (S.Y. Park et al., Prevention of Urban Crime Using CPTED, Korea: Journal of the Sociality of Living System, 17(4), 2010.04, pp.20-22.)

[4] 이민아, 김민정, 신지현, 아파트 단지 내 사회적 경제 디자인기법 적용, 한국: 한국건축학회지회연합회 학술발표대회논문집, 1975(1), 1975.12, pp.2-5. // (M.A. Lee, M.J. Kim, J.H. Shin, Apartment Complex to Application of the Social Economy Design, Korea: Conference Journal of AIROKRA, 1975(1), 1975.12, pp.2-5.)

[5] T. Johnson, Crime Prevention Through Environmental Design Applications of Architectural Design and Space Management Concepts, Second Edition, Canada: National Crime Prevention Institute, 2000, pp.333-356.

[6] B. Pitt et al., The Science and Politics of Early Event Prevention: The Asian Experience and Directions for New York, Raleigh: Duke Press, 1999, pp.75-76.

[7] Korea Institute of Ecological Architecture and Environment Journal, Paper format, http://www.kieae.org/abcd, 2019.02.02.